**TEMPOSTOP 3 time flow basin tap**

(AB) Anti-blocking model

Reinforced fixings

Reference: **703000AB**

Specification description

Deck-mounted push-button basin tap:

Time flow ~7 seconds.

Pre-set flow rate 3 lpm at 3 bar, adjustable from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Chrome-plated brass body M½".

Fixing reinforced by back-nut.

AB anti-blocking system: water only flows when push-button is released

30-year warranty.