**TEMPOMATIC electronic basin tap**

Mains supply

CW ≤ 30mm

Reference: **441100**

Specification description

Cross wall electronic basin tap:

Independent IP44 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Chrome-plated fixed spout L. 170mm with anti-rotating pin and back-nut.

Escutcheon flush to the wall.

Shockproof infrared presence detection sensor.

Anti-blocking security.

For panels ≤ 30mm.

Solenoid valve M 3/8" with integrated filter.

Threaded rods can be cut to size.

Suitable for People with Reduced Mobility.

30-year warranty.