**SECURITHERM sequential thermostatic shower mixer**

Thermostatique mixer with no non-return valves, bottom outlet

Without unions

Reference: **9630**

Specification description

SECURITHERM sequential thermostatic shower mixer.

Sequential thermostatic mixer: opens and closes with cold water.

Mixer with no non-return valves on the inlets (reduces bacterial proliferation).

No risk of cross flow between the hot and cold water.

Sequential mixer with anti-scalding failsafe: shuts off automatically if cold water supply fails.

Prevents cold showers: shuts off automatically if hot water supply fails.

Securitouch thermal insulation prevents burns.

Scale-resistant sequential thermostatic cartridge adjusts the flow rate and the temperature.

Temperature adjusts from cold water up to 39°C with temperature limiter set at 39°C.

Thermal shocks are possible.

Body with smooth interior and low water volume (reduces bacterial proliferation).

Flow rate regulated at 9 l/min.

Chrome-plated brass body and Hygiene lever L. 100mm.

M1/2" bottom outlet.

Mixer with no wall connectors with filters integrated in the inlets, F3/4".

Mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Sequential mixer suitable for people with reduced mobility.

Shower mixer with 30-year warranty.