**Divider for L trough urinal**

304 polished satin stainless steel - H. 1020mm

Reference: **100910**

Specification description

Divider for recessed L trough urinal.

304 bacteriostatic stainless steel.

Polished satin stainless steel.

Stainless steel thickness: 3mm.

Install directly onto the urinal in the desired position.

Only suitable for recessed L trough urinals refs 130200, 130210 et 130220.

Weight: 3.9kg.

30-year warranty.