**Divider for LP trough urinal**

Polished satin 304 stainless steel - H. 770mm

Divider for LP trough urinal

Reference: **100920**

Specification description

Divider for floor-standing LP trough urinal.

304 stainless steel.

Polished satin finish.

Stainless steel thickness: 3mm.

Install directly onto the urinal in the desired position.

Only suitable for floor-standing LP trough urinals refs 130300, 130310 and 130320.

Weight: 2.75kg.

30-year warranty.