**Cross-wall tamperproof controls ≤ 200mm**

For cross-wall showers and basin controls

Reference: **749TC200**

Specification description

Cross-wall tamperproof controls ≤ 200mm, chrome-plated metal.

With anti-rotating pin and back-nut.