**Lift-up shower seat with leg**

Wall-mounted lift-up shower seat with solid seat

White powder-coated aluminium structure

Reference: **510405**

Specification description

Lift-up shower seat with leg.

Shower seat for disabled people and people with reduced mobility.

Non-slip solid seat made from polypropylene.

Seat is comfortable and easy to maintain.

Hinged leg which folds automatically.

Structure made from white aluminium tubing, Ø 25 x 2mm.

Concealed fixings.

Dimensions 410 x 360 x 480mm.

Folded dimensions: 85mm.

Seat height: 480mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

Wall-mounted lift-up shower seat with 30-year warranty. CE marked.