**Automatic hand dryer activated via optical cell, 304 stainless steel**

Optical cell

304 bright polished stainless steel

Reference: **6631**

Specification description

Automatically activated by optical cell.

304 stainless steel cover, bright polished finish.

Dimensions: 124 x 216 x 318mm.

Weight: 3.8kg.

Power: 1,960W. 50 Hz.

Airflow: 65 l/second.

Flow noise level: 58 dBA.

Class I, IPX1.

CE marked, TÜV GS.

3-year warranty.