**Self-adhesive rectangular stainless steel mirror, H. 600mm**

Unbreakable mirror

"Mirror" polished 304 stainless steel

Reference: **3453**

Specification description

Wall-mounted rectangular, "mirror" polished bacteriostatic 304 stainless steel mirror.

Stainless steel thickness: 1mm.

Self-adhesive.

For installation on a flat surface.

Unbreakable mirror.

Dimensions: 1 x 600 x 400mm.

30-year warranty.