**Wall-mounted liquid soap dispenser, 1.2 litres**

Hypereco

Bright polished 304 stainless steel

Reference: **6567**

Specification description

Wall-mounted liquid soap dispenser.

Bacteriostatic bright polished 304 stainless steel.

One piece.

With lock.

Capacity: 1.2 litres.

Level control.

Concealed fixings.

Refill trap hinged at the top.

Dimensions: 70 x 125 x 210mm.

Possible to order the valve assembly (ref. 6568) and a control level window (ref. 6569) separately.

Wall-mounted soap dispenser with a 30-year warranty.