**Angled curtain rail**

Rotate to adjust size

From 0.70 - 0.90m

Reference: **362**

Specification description

Extendable, angled curtain rail.

Angled rod for shower curtains made from bright polished 304 stainless steel.

Tube Ø 20mm and Ø 16mm, 1mm thick

Can be adjusted from 0.70 - 0.90m on either side.

Simply rotate the tube to adjust.

30-year warranty.