**Chrome-plated shower rail**

With soap dish and hose retaining collar

Ø 25mm rail

Reference: **821**

Specification description

Chrome-plated stainless steel shower rail Ø 25mm, overall length 632mm, centres can be adjusted up to 602mm, can be cut to size.

Adjustable, tilting chrome-plated shower head holder.

Shower hose retaining collar.

Chrome-plated soap dish.