**Single hole mixer - 100 lpm**

Mixer with high flow rate for plunge sinks

Reference: **5610**

Specification description

Deck-mounted single hole mixer for professional catering.

Mixer for plunge sinks with swivelling, tubular spout H. 315mm L. 300mm.

Star-shaped, brass flow straightener.

Water-free guided valve heads with reinforced mechanisms.

Shock-resistant, ergonomic ball levers.

Flow rate 100 lpm at 3 bar suitable for plunge sinks.

Full flow rate within half a turn.

Spout with smooth interior.

Chrome-plated brass body and spout.

Soldered copper pipe water inlets.

Reinforced fixings.

Suitable for intensive use in professional kitchens.

30-year warranty.