**Standard oven cleaner**

With push-button

Reference: **D275059**

Specification description

Oven cleaner with stopcock and ceramic discs with:

Integrated back-flow prevention device and non-return valve.

White, opaque reinforced PVC flexible hose FF1/2", L. 1.25m.

Push-button operated hand spray.

Chrome-plated, wall-mounted brass hook.

30-year warranty.

It is possible to fit a time flow valve.