**TEMPOGENOU time flow tap**

Knee-operated

Angled model

Reference: **734100**

Specification description

Knee-operated time flow basin valve:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Reinforced control lever.

Wall-mounted chrome-plated fixing plate.

Cold or mixed water supply.

Chrome-plated brass body M½".

Angled model for wall inlet M½".

30-year warranty.