**Fixed tubular spout**

L.150mm, H.170mm

Deck-mounted

Reference: **204001**

Specification description

Tubular spout Ø 16mm, M½".

L. 150mm, H. 170mm

Chrome-plated brass.

Spout with smooth interior (reduces niches where bacteria can develop).

Scale-resistant flow straightener regulated at 3 lpm.

30-year warranty.