**TEMPOSOFT time flow shower panel**

Time flow, aluminium

Top inlet, handset, aluminium

Reference: **749350**

Specification description

Time flow shower panel:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Top inlet supply for mixed water via in-line stopcock M½".

TEMPOSOFT time flow control for mixed water.

Soft-touch operation.

Time flow ~30 seconds.

Sliding handset on chrome-plated rail with flexible.

Concealed fixings.

Filter.

Suitable for people with reduced mobility.

30-year warranty.