**Recessed tube inlet**

For siphon or standard urinal

F½", Ø 35mm

Reference: **758135**

Specification description

Recessed inlet for siphon action or standard urinal

F½", Ø 35mm.

30-year warranty.