**Corner wedge**

For urinals IDEAL STANDARD, JACOB DELAFON, LAUFEN or PORCHER

L. 35mm

Reference: **770035**

Specification description

Corner wedge L.35 mm for:

TEMPOSTOP (ref. 777000)

or TEMPOSOFT 2 (ref. 778800).

For angle-mounted urinals IDEAL STANDARD "Applique 3874", JACOB DELAFON "Coquille 2 1516", LAUFEN "Como" or PORCHER "Applique 2651".

30-year warranty.