**REDO-T floor-standing washbasin**

Polished satin 304 stainless steel

With Ø 35mm central tap hole

Reference: **121720**

Specification description

Floor-standing washbasin, height 830mm. Basin internal diameter: 310mm.

Design-led styling.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 0.8mm.

Rounded edges prevent injury.

With Ø 35mm central tap hole.

Supplied with 1¼" waste. Without overflow.

Supplied with fixings.

CE marked. Complies with European standard EN 14688.

Weight: 14kg.

30-year warranty.