**Wall-mounted cleaners' sink**

Polished satin 304 stainless steel - L. 460mm

Reference: **182400**

Specification description

Wall-mounted sink with splashback.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 0.9mm.

Seam-free, pressed bowl.

Deep sink.

Smooth surface.

Rounded edges prevent injury.

Supplied with 1½" waste .

Without overflow.

Supplied with fixing elements and splashback.

Can install with a stainless steel hinged grid (ref 102400).

Weight: 4.6kg.

30-year warranty.