**Surgical scrub-up trough with high upstand**

Polished satin 304 stainless steel - 2 services - "Hygiene+" Design

Without tap hole

Reference: **186000**

Specification description

Wall-mounted surgical scrub-up trough with 450mm upstand.

Suitable for hospitals and healthcare facilities.

Bacteriostatic 304 stainless steel. Polished satin finish. Stainless steel thickness: 1.2mm.

Length 1,400mm, 2 services. Without tap hole.

Smooth surface and rounded inside edges for easy cleaning.

"Hygiene+" design: reduces niches where bacteria can develop, concealed trap, easy to clean.

Drainage on the right. Without overflow. Supplied with fixing elements and 1"1/4 waste.

CE marked. Complies with norm EN 14296.

Weight: 34.4kg.

30-year warranty.