**MINI BAILA wall-mounted washbasin**

Dual finish 304 stainless steel

Without tap hole

Reference: **120182**

Specification description

Wall-mounted washbasin. Basin internal diameter: 310mm.

Design-led styling.

Bacteriostatic 304 stainless steel.

Dual finish: bright polished basin interior and polished satin exterior.

Stainless steel thickness: 1mm.

Rounded edges prevent injury.

Without tap hole.

Supplied with 1¼" waste. Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 4.1kg.

30-year warranty.