**BIOSAFE polyurethane flexible hose**

For retracting hand spray

Reference: **837T4**

Specification description

BIOSAFE flexible hose L. 1.60m reduces bacterial proliferation, for retracting hand sprays (except ref. 2597).

Polyurethane transparent flexible hose with smooth interior and exterior and low water capacity (interior Ø 6mm).

Metal conical union F1/2".