**Basic drop-down support rail, white, L. 760 mm, with leg**

White powder-coated stainless steel

Ø 32mm

Reference: **511517W**

Specification description

Basic drop-down support rail Ø 32mm with leg, for people with reduced mobility.

Basic drop-down grab bar made from white powder-coated stainless steel for WCs or showers.

Model with automatic folding leg: to be used as a reinforcement when the wall fixing alone is insufficient.

Leg height can be adjusted from 760 to 780mm.

Visible fixings, secured to wall by a 6-hole plate.

Wall plate thickness: 3.5mm.

Dimensions: 760 x 815 x 100mm.

30-year warranty.

CE marked.