**Cover plate for Be-Line drop-down rail**

Metallised anthracite

Without fixing plate

Reference: **511950C**

Specification description

Cover plate for Be-Line® drop-down rails.

Conceals fixing screws when the drop-down support rail is removed.

Reduces the number of drop-down rails in a facility, allowing installation only when required.

Example: hotels or hospitals providing short-term accommodation for people with reduced mobility.

Metallised anthracite cover without fixing plate.

30-year warranty.