**Surgical scrub-up trough with low upstand**

Polished satin 304 stainless steel - 3 services - L. 2,400mm

Without tap hole - "Hygiène +" Design

Reference: **18702015**

Specification description

Wall-mounted surgical scrub-up trough with 75mm upstand.

Suitable for hospitals and care facilities.

Complies with the former HTM64 guidance and new Health Building Note 00-10: Part C - Sanitary Assemblies.

Length 2,400mm, 3 services. Without tap hole.

Bacteriostatic 304 stainless steel. Polished satin finish. Stainless steel thickness: 1.2mm.

Smooth surface and rounded edges for easy cleaning.

"Hygiene +" design: reduces bacterial niches, concealed trap, easy to clean.

Drainage on the right. Without overflow. Supplied with fixing elements.

CE marked. Complies with norm EN 14296.

Weight: 42.5kg.

30-year warranty.