**ECO aerator**

1.4 lpm

M16.5/100

Reference: **925716.2P**

Specification description

Rain effect aerator.

1.4 lpm.

M16.5/100 to screw in.

Complies with environmental label requirements.

Supplied in packs of 2.

30-year warranty.