**Twin hole pre-rinse set with mixer**

Without bib tap

White flexible and scale-resistant hand spray

Reference: **G6833**

Specification description

Complete pre-rinse set with bib tap suitable for intensive use in professional kitchens.

Deck-mounted twin hole mixer with adjustable centres 100 - 240mm with:

- valve heads with control knobs.

- offset inlet connections with M1/2" tails.

White hand spray with adjustable jet and 10 lpm flow rate at the outlet (ref. 433003).

Scale-resistant hand spray with shock-resistant tip.

Reinforced, food-grade, white flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.

These pre-rinse models can be installed close to the splashback.