**Black pre-rinse set without valve with short column**

With bib tap and swivelling tubular spout

Black flexible and scale-resistant hand spray

Reference: **435622**

Specification description

Black pre-rinse set without valve suitable for intensive use in professional kitchens.

Bib tap with swivelling tubular spout L. 200mm.

- full flow rate within 1/4-turn.

- valve head with reinforced mechanism and ergonomic control.

Black hand spray with adjustable jet with 10 lpm at the outlet (ref. 433009).

Scale-resistant hand spray with shock-resistant tip.

Reinforced, food-grade, black flexible hose L. 0.95m.

3/4" short brass column for wall-mounted water control valve.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.

This model, without water control valve, comprises spare parts for refurbishing pre-rinse sets.