**LAVANDO WC hand washbasin**

Polished satin 304 stainless steel

With Ø35mm tap hole on left side

Reference: **121360**

Specification description

WC hand washbasin, 450 x 300mm.

Design-led hand washbasin.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

With tap hole Ø35mm on left side.

Supplied with waste 1¼".

Without overflow.

Supplied with fixings.

CE marked. Complies with norm EN 14688.

Weight: 3.2kg.