**Recessed waterproof housing for TEMPOSTOP shower**

Recessed, kit 1/2

Waterproof

Reference: **749BOX**

Specification description

Recessed waterproof housing, kit 1/2.

For TEMPOSTOP shower.

Partition thickness can be between 10 to 30mm.

30-year warranty.

Order with control plate reference 749218 or with shower kit reference 749239.