**Electronic control unit**

For TEMPOMATIC WC dual control

Cartridge and solenoid valve

Reference: **461032**

Specification description

Electronic control unit: cartridge and solenoid valve.

Dual control.

Connection: 1 1/4"

Dimensions: Ø 4mm

For TEMPOMATIC WC dual control.