**TEMPOMATIC 4 deck-mounted electronic soap dispenser**

Liquid or foam soap or hydroalcoholic gel dispenser

Mains, chrome-plated 304 stainless steel, 1L tank

Reference: **512031P**

Specification description

Deck-mounted electronic soap dispenser.

Liquid soap, mousse or hydroalcoholic gel dispenser.

No manual contact: hands are automatically detected by infrared cell.

Chrome-plated 304 stainless steel spout.

No-waste pump dispenser.

Removable, separate electronic unit and tank for installation beneath the work surface.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s. or special foam soap.

Compatible with hydroalcoholic gel.

Spout length: 111mm.

Supplied with a 1-litre tank.

30-year warranty.

CE marked.