**Ø40mm ceramic cartridge**

Cartridge without base

With flow rate limiter

Reference: **N248AA75**

Specification description

Ø40 standard ceramic cartridge with no base, with flow rate limiter.

Cartridge for the 2522 range.