**Non-return valve**

For 3/8" connections

Reference: **900010**

Specification description

Non-return valve for 3/8" connections for basin and sink mixers.

Ø 10mm non-return valve prevents back flow of foul water in the system.

Prevents any cross flow of cold/hot water.