**Non-return valve**

Ø 15mm non-return valve

Reference: **900015**

Specification description

Non-return valve for basin and shower mixers.

Ø 15mm non-return valve prevents any backflow of contaminated water into the system.

Prevent cross flow of cold and hot water.