**Time flow cartridge**

Mechanism for TEMPOCHASSE WC

~7sec time flow

Reference: **743779**

Specification description

Time flow cartridge for TEMPOCHASSE WC valve

With push-button.

For 3/4" WC.

Time flow ~7 seconds.

Base flow rate: 1 L/sec at 1 bar dynamic pressure.