**Time flow cartridge**

Mechanism for TEMPOSTOP urinal

Time flow ~3 seconds

Reference: **743003**

Specification description

Time flow cartridge for TEMPOSTOP urinal valve.

Old design.

For 1/2" valve.

With push-button.

Time flow ~3 seconds.

Adjustable flow rate.