**Time flow cartridge**

Mechanism for TEMPOFLUX WC

Time flow ~7 seconds

Reference: **743763**

Specification description

Time flow cartridge for TEMPOFLUX WC valve

For recessed or TC 3/4" WC valves.

Time flow ~7 seconds.