**Thermostatic cartridge for shower mixers**

SECURITHERM thermostatic sequential cartridge

For H9630/H9640 shower mixers

Reference: **N963**

Specification description

Thermostatic sequential cartridge for exposed thermostatic shower mixers.

SECURITHERM cartridge for H9630/H9640 mixers.

To replace cartridge N9630.