**Maintenance kit for basin cartridge**

For wall-mounted TEMPOMIX basin

Time flow ~7 seconds

Reference: **753796**

Specification description

Cartridge maintenance kit for wall-mounted TEMPOMIX basin mixer/tap.

Temporisation ~7 s.