**Refit kit for basin/urinal cartridge**

For TEMPOSTOP basin/urinal

Time flow ~7 seconds, AB anti-blocking system

Reference: **753105**

Specification description

Refit kit for TEMPOSTOP basin/urinal time flow cartridge.

Time flow ~7 seconds.

AB anti-blocking system.

Until 2022.