**Time flow cartridge**

For TEMPOSTOP 2 and TEMPOMIX 2 basin

Time flow ~7 seconds, AB anti-blocking system

Reference: **743908**

Specification description

Time flow cartridge for TEMPOSTOP 2 and TEMPOMIX 2 basin.

Time flow ~7 seconds.

AB anti-blocking system.