**Hand spray with inverter**

Hand spray with flow rate regulator valve

For mixers with retracting hand sprays

Reference: **817**

Specification description

Shower hand spray M1/2" Ø 60mm with automatic inverter.

Hand spray with flow rate regulator valve in chrome-plated ABS.

2 jets: rain effect and massage.