**TEMPOSTOP 3 time flow basin tap**

Wall-mounted, 3/8"

Reference: **703201**

Specification description

Wall-mounted push-button basin tap:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, adjustable from 1.4 to 6 lpm.

Vandal-resistant scale-resistant flow straightener.

Chrome-plated solid brass body M3/8".

30-year warranty.