**Dual flush button 3L/6L for TEMPOFLUX 2**

Dual flush for TEMPOFLUX 2 WC

Reference: **762BUT3**

Specification description

Dual flush button 3L/6L for cistern-less WC system TEMPOFLUX 2.

Fixed with hidden screws.

Ø 64mm.