**Single flush button 6L for TEMPOFLUX 2**

For single flush TEMPOFLUX 2 WC

Reference: **762BUT6**

Specification description

Single flush button 6L for cistern-less WC system TEMPOFLUX 2.

Fixed with hidden screws.

Ø 65mm.