**Electronic control unit**

For TEMPOMATIC 4

Battery operated

Reference: **490454**

Specification description

Electronic control unit.

For TEMPOMATIC 4.

Power supplied by 6V batteries (included).

Dimensions: 56mm, Ø 51mm.