**Designer toilet seat lid with soft close**

For BCN models

Black Duroplast

Reference: **103419**

Specification description

Toilet seat with lid.

Made from Duroplast.

With 304 stainless steel hinges.

Slimline design.

Soft close toilet seat lid: slow closure, gently and silently.

Toilet seat lid can be removed: easy to install and remove for thorough and effective cleaning.

Colour: black.

For BCN WC models.

Supplied with fixing elements.

30-year warranty.